Cable Raceway
240*100mm series

Applications
PROSE optical fiber raceway is a set of products that can provide full protection for optical fibers and facilitate operation. The basic components include: channel body, connectors, horizontal elbows, vertical elbows, horizontal tees, horizontal crosses, vertical tees, adapters, terminal end caps, fiber outlets, bell mouths, and various support components. Featuring a standardized modular design with high engineering precision, it offers rapid, flexible, and comprehensive protection for optical fibers.

Characteristic 
· Innovative design, full arc dead angle protection fiber optic cable.
· Tool-free installation, barrier-free connection.
· Multiple fiber outlet specifications to meet fiber requirements in various locations.
· Powerful compatibility, worry-free expansion.
· UL94-V0 highest-level flame-retardant material.



Straight.Duct
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	Product Number
	[bookmark: OLE_LINK1]CR24-SD-111-11(Body) CR24-SD-110-11(Cover)

	Size
	240mm (W) x 100mm (H) x 2000(mm) (L)

	Flame retardant level
	UL94-V0

	External dimensions
	Body: 1278×118×2000(mm), Cover: 274×12×2000(mm)

	Maximum payout
	5800 strands (3 mm wire)



Duct Connector 
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	Product Number
	CR24-CO-211-11

	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Connection of components of 240-width Straight Duct

	External dimensions
	287×60×119(mm)

	Installation requirements
	PR-LT5B4 Plastic round handle bolt ×8



Horizontal Corner Bend 
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	Product Number
	CR24-CB-311-11(Body), CR24-CB-310-11 (Cover)

	Specification dimensions
	[bookmark: OLE_LINK4]240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct horizontal turns

	External dimensions
	Body: 347×347×121(mm), Cover: 381×381×37(mm)

	Installation requirements
	2 sets of fittings; cover plate optional





Horizontal Tee 
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	Product Number
	CR24-TE-411-11(Body), CR24-TE-410-11 (Cover)

	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct horizontal T-shaped connection

	External dimensions
	Body: 410×347×121(mm), Cover: 480×381×37(mm)

	Installation requirements
	3 sets of fittings; cover optional




Horizontal Cross
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	Product Number
	CR24-CR-511-11(Body), CR24-CR-510-11 (Cover)

	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct horizontal Cross

	External dimensions
	Body: 410×410×121(mm), Cover: 480×480×37 (mm)

	Installation requirements
	4 sets of fittings; cover optional



End Closure
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	Product Number
	CR24-EC-611-11


	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct End Closure

	External dimensions
	270×25×116(mm)

	Installation requirements
	1 PR-LT5B4 Plastic round handle bolt ×4
2 PR-LT338 Plastic square nut ×4



45° Upward Elbow
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	Product Number
	CR24-AE-710-11 (Cover)

	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct 45° Upward Elbow

	External dimensions
	Body: 320×287×121(mm), Cover: 290×325×40(mm)

	Installation requirements
	2 sets of fittings; cover optional


45° Upward Elbow
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	Product Number
	[bookmark: OLE_LINK7]CR24-AE-711-11(Body)

	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct 45° Upward Elbow

	External dimensions
	Body: 320×287×121(mm), Cover: 290×325×40(mm)

	Installation requirements
	2 sets of fittings; cover optional
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	Product Number
	CR24-AE-720-11 (Cover)

	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct 45° Downward Elbow

	External dimensions
	Body: 277×187×162(mm), Cover: 286×199×100(mm)

	Installation requirements
	2 sets of fittings; cover optional


45° Downward Elbow
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	Product Number
	CR24-AE-721-11(Body)

	Specification dimensions
	240×100(mm)

	Flame retardant level
	UL94-V0

	Scope of application
	Applicable to 240 series Straight Duct 45° Downward Elbow

	External dimensions
	Body: 277×187×162(mm), Cover: 286×199×100(mm)

	Installation requirements
	2 sets of fittings; cover optional



Waterfall Outlet 
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	Series
	90*170mm Series
	120*170mm Series
	130*170mm Series

	Product Number(Body)
	CRAC-WO-851-11
	CRAC-WO-861-11
	CRAC-WO-871-11

	Product Number(Cover)
	CRAC-WO-850-11
	CRAC-WO-860-11
	CRAC-WO-870-11

	External dimensions(Body)
	186×170×130mm
	250×211×146mm
	226×170×130mm

	External dimensions(Cover)
	108×103×153mm
	258×260×149mm
	148×103×153mm

	Flame retardant level
	UL94-V0
	UL94-V0
	UL94-V0

	Color
	Yellow
	Yellow
	Yellow

	Materials
	PVC / ABS
	PVC / ABS
	PVC / ABS

	Corrugated Tube Size
	55mm
	55mm/80mm
	55mm/80mm

	Installation requirements
	Round Plastic Screw with Nut ×2set
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	Product Number
	CRACT-911-11(Φ55mm), CRACT-921-11(Φ80mm)


	Color
	Yellow

	Materials
	PVC / ABS

	Installation requirements
	Position fixer×1set




Screw and Nut
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	Product Number
	CRAC-SN-211-11/CRAC-SN-221-11
CRAC-SN-221-11
CRAC-SN-221-11
CRAC-SN-221-11

CRAC-SN-221-11
CRAC-SN-221-11
CRAC-SN-221-11
CRAC-SN-221-11

CRAC-SN-221-11

/

	Specification dimensions(mm)
	M5×12(Screw); M5(Nut)

	External dimensions(mm)
	Φ25×24mm (Screw); 19×13x2.5mm (Nut)



 
Supporting Assembly 
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	Product Number
	CRAC-SA-XXX-XX

	Accessories
	1 T-shaped Plastic Screw ×2
2 Plastic knob Nut × 2
3 “U” types of overhead cranes × 2
4 Plastic double-hole crossarm × 1
5 Expansion screws × 4
6 Threaded rod × 2
7 Flange nuts × 8
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