[bookmark: _Hlk107930653]FTTH Fiber Distribution BOX
FDB-481 Series

[bookmark: _Hlk107930639]Application
Prose FTTH Fiber Distribution Box is designed for fiber termination, distribution, and management in access networks. It supports fiber splicing, splitting, storage, and subscriber connection. Suitable for both indoor and outdoor installations, it is widely used in residential, commercial, and FTTH deployment scenarios.
Key Features
· Supports up to 48 fiber cores for high-density FTTH applications
· Integrated design for splicing, splitting, routing, and storage
· Multiple cable entry ports for feeder and drop cable flexibility
· Made of high-strength flame-retardant material with reliable protection
· Supports wall-mounted and pole-mounted installation methods
Product Appearance
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Technical Parameters
	[bookmark: _Hlk148294607]Material
	ABS, PC+ABS

	Dimensions
	355 × 270 × 120 mm

	Fiber Capacity
	24F / 48F

	Capacity
	Supports up to 48 fiber adapters and pigtails

	Waterproof Rating
	IP65, IP66

	Color
	White, Black

	Storage temperature range
	-40°C to +70°C

	Installation temperature range	
	-10°C to +60°C


Ordering Information	
	Part Number
	Description

	FBD-481-E
	FTTH Fiber Distribution Box, 48 Port, White, Unloaded

	FBD-481-SCGD1
	FTTH Fiber Distribution Box, 48 Port, with 48pcs SM SC Adapter & 48pcs SC SM Pigtail
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